inorganic_metal

[OBJECT:INORGANIC]

Dwarfoloid picked out a lot of the material numbers here to replace my placeholders.

[INORGANIC:IRON]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:iron]
	[STATE_NAME_ADJ:LIQUID:molten iron]
	[STATE_NAME_ADJ:GAS:boiling iron]
	[DISPLAY_COLOR:0:7:1]
	[MATERIAL_VALUE:10]
	[SPEC_HEAT:450]
	[MELTING_POINT:12768]
	[BOILING_POINT:15150]
	[ITEMS_WEAPON][ITEMS_WEAPON_RANGED][ITEMS_AMMO][ITEMS_DIGGER][ITEMS_ARMOR][ITEMS_ANVIL]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]
	[SOLID_DENSITY:7850]
	[LIQUID_DENSITY:6980]
	[MOLAR_MASS:55845]
	[IMPACT_YIELD:542500] Was 1080000, but just using 3.5x tensile multiples for everything until better numbers are available, which might not be likely
	[IMPACT_FRACTURE:1085000]
	[IMPACT_STRAIN_AT_YIELD:319]
	[COMPRESSIVE_YIELD:542500]
	[COMPRESSIVE_FRACTURE:1085000]
	[COMPRESSIVE_STRAIN_AT_YIELD:319] bulk modulus 170 GPa
	[TENSILE_YIELD:155000]
	[TENSILE_FRACTURE:310000]
	[TENSILE_STRAIN_AT_YIELD:73] young's modulus 211 GPa
	[TORSION_YIELD:155000]
	[TORSION_FRACTURE:310000]
	[TORSION_STRAIN_AT_YIELD:189]
	[SHEAR_YIELD:155000]
	[SHEAR_FRACTURE:310000]
	[SHEAR_STRAIN_AT_YIELD:189] shear modulus 82 GPa
	[BENDING_YIELD:155000]
	[BENDING_FRACTURE:310000]
	[BENDING_STRAIN_AT_YIELD:73]
	[MAX_EDGE:10000]

[INORGANIC:GOLD]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME:SOLID:gold]
	[STATE_NAME:SOLID_POWDER:gold dust]
	[STATE_ADJ:ALL_SOLID:gold]
	[STATE_NAME_ADJ:LIQUID:molten gold]
	[STATE_NAME_ADJ:GAS:boiling gold]
	[DISPLAY_COLOR:6:6:1]
	[MATERIAL_VALUE:30]
	[SPEC_HEAT:129]
	[MELTING_POINT:11915]
	[BOILING_POINT:15141]
	[SOLID_DENSITY:19320]
	[LIQUID_DENSITY:17310]
	[MOLAR_MASS:196967]
	[IMPACT_YIELD:175000]
	[IMPACT_FRACTURE:350000]
	[IMPACT_STRAIN_AT_YIELD:97]
	[COMPRESSIVE_YIELD:175000]
	[COMPRESSIVE_FRACTURE:350000]
	[COMPRESSIVE_STRAIN_AT_YIELD:97] bulk modulus 180 GPa
	[TENSILE_YIELD:50000]
	[TENSILE_FRACTURE:100000]
	[TENSILE_STRAIN_AT_YIELD:64] young's modulus 78 GPa
	[TORSION_YIELD:50000]
	[TORSION_FRACTURE:100000]
	[TORSION_STRAIN_AT_YIELD:185]
	[SHEAR_YIELD:50000]
	[SHEAR_FRACTURE:100000]
	[SHEAR_STRAIN_AT_YIELD:185] shear modulus 27 GPa
	[BENDING_YIELD:50000]
	[BENDING_FRACTURE:100000]
	[BENDING_STRAIN_AT_YIELD:64]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:SILVER]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:silver]
	[STATE_NAME_ADJ:LIQUID:molten silver]
	[STATE_NAME_ADJ:GAS:boiling silver]
	[DISPLAY_COLOR:7:7:1]
	[MATERIAL_VALUE:10]
	[SPEC_HEAT:230]
	[MELTING_POINT:11731]
	[BOILING_POINT:13892]
	[ITEMS_WEAPON][ITEMS_AMMO]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]
	[SOLID_DENSITY:10490]
	[LIQUID_DENSITY:9320]
	[MOLAR_MASS:107868]
	[IMPACT_YIELD:350000]
	[IMPACT_FRACTURE:595000]
	[IMPACT_STRAIN_AT_YIELD:350]
	[COMPRESSIVE_YIELD:350000]
	[COMPRESSIVE_FRACTURE:595000]
	[COMPRESSIVE_STRAIN_AT_YIELD:350] 100
	[TENSILE_YIELD:100000]
	[TENSILE_FRACTURE:170000]
	[TENSILE_STRAIN_AT_YIELD:120] 83
	[TORSION_YIELD:100000]
	[TORSION_FRACTURE:170000]
	[TORSION_STRAIN_AT_YIELD:333]
	[SHEAR_YIELD:100000]
	[SHEAR_FRACTURE:170000]
	[SHEAR_STRAIN_AT_YIELD:333] 30
	[BENDING_YIELD:100000]
	[BENDING_FRACTURE:170000]
	[BENDING_STRAIN_AT_YIELD:120]
	[MAX_EDGE:10000]

[INORGANIC:COPPER]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:copper]
	[STATE_NAME_ADJ:LIQUID:molten copper]
	[STATE_NAME_ADJ:GAS:boiling copper]
	[DISPLAY_COLOR:6:4:0]
	[MATERIAL_VALUE:2]
	[SPEC_HEAT:385]
	[MELTING_POINT:11952]
	[BOILING_POINT:14611]
	[ITEMS_WEAPON][ITEMS_WEAPON_RANGED][ITEMS_AMMO][ITEMS_DIGGER][ITEMS_ARMOR]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]
	[SOLID_DENSITY:8930]
	[LIQUID_DENSITY:8020]
	[MOLAR_MASS:63546]
	[IMPACT_YIELD:245000]
	[IMPACT_FRACTURE:770000]
	[IMPACT_STRAIN_AT_YIELD:175]
	[COMPRESSIVE_YIELD:245000]
	[COMPRESSIVE_FRACTURE:770000]
	[COMPRESSIVE_STRAIN_AT_YIELD:175] 140
	[TENSILE_YIELD:70000]
	[TENSILE_FRACTURE:220000]
	[TENSILE_STRAIN_AT_YIELD:58] 120
	[TORSION_YIELD:70000]
	[TORSION_FRACTURE:220000]
	[TORSION_STRAIN_AT_YIELD:145]
	[SHEAR_YIELD:70000]
	[SHEAR_FRACTURE:220000]
	[SHEAR_STRAIN_AT_YIELD:145] 48
	[BENDING_YIELD:70000]
	[BENDING_FRACTURE:220000]
	[BENDING_STRAIN_AT_YIELD:58]
	[MAX_EDGE:10000]

[INORGANIC:NICKEL]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:nickel]
	[STATE_NAME_ADJ:LIQUID:molten nickel]
	[STATE_NAME_ADJ:GAS:boiling nickel]
	[DISPLAY_COLOR:7:3:0]
	[MATERIAL_VALUE:2]
	[SPEC_HEAT:444]
	[MELTING_POINT:12619]
	[BOILING_POINT:15243]
	[SOLID_DENSITY:8800]
	[LIQUID_DENSITY:7810]
	[MOLAR_MASS:58693]
	[IMPACT_YIELD:70000]
	[IMPACT_FRACTURE:560000]
	[IMPACT_STRAIN_AT_YIELD:39]
	[COMPRESSIVE_YIELD:70000]
	[COMPRESSIVE_FRACTURE:560000]
	[COMPRESSIVE_STRAIN_AT_YIELD:39] 180
	[TENSILE_YIELD:20000]
	[TENSILE_FRACTURE:160000]
	[TENSILE_STRAIN_AT_YIELD:10] 200
	[TORSION_YIELD:20000]
	[TORSION_FRACTURE:160000]
	[TORSION_STRAIN_AT_YIELD:26]
	[SHEAR_YIELD:20000]
	[SHEAR_FRACTURE:160000]
	[SHEAR_STRAIN_AT_YIELD:26] 76
	[BENDING_YIELD:20000]
	[BENDING_FRACTURE:160000]
	[BENDING_STRAIN_AT_YIELD:10]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:ZINC]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:zinc]
	[STATE_NAME_ADJ:LIQUID:molten zinc]
	[STATE_NAME_ADJ:GAS:boiling zinc]
	[DISPLAY_COLOR:7:3:0]
	[MATERIAL_VALUE:2]
	[SPEC_HEAT:390]
	[MELTING_POINT:10755]
	[BOILING_POINT:11633]
	[SOLID_DENSITY:7135]
	[LIQUID_DENSITY:6570]
	[MOLAR_MASS:65380]
	[IMPACT_YIELD:175000]
	[IMPACT_FRACTURE:525000]
	[IMPACT_STRAIN_AT_YIELD:250]
	[COMPRESSIVE_YIELD:175000]
	[COMPRESSIVE_FRACTURE:525000]
	[COMPRESSIVE_STRAIN_AT_YIELD:250] 70
	[TENSILE_YIELD:50000]
	[TENSILE_FRACTURE:150000]
	[TENSILE_STRAIN_AT_YIELD:46] 108
	[TORSION_YIELD:50000]
	[TORSION_FRACTURE:150000]
	[TORSION_STRAIN_AT_YIELD:116]
	[SHEAR_YIELD:50000]
	[SHEAR_FRACTURE:150000]
	[SHEAR_STRAIN_AT_YIELD:116] 43
	[BENDING_YIELD:50000]
	[BENDING_FRACTURE:150000]
	[BENDING_STRAIN_AT_YIELD:46]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:BRONZE]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:bronze]
	[STATE_NAME_ADJ:LIQUID:molten bronze]
	[STATE_NAME_ADJ:GAS:boiling bronze]
	[DISPLAY_COLOR:6:4:0]
	[MATERIAL_VALUE:5]
	[SPEC_HEAT:435]
	[MELTING_POINT:11868]
	[BOILING_POINT:14140]
	[ITEMS_WEAPON][ITEMS_WEAPON_RANGED][ITEMS_AMMO][ITEMS_DIGGER][ITEMS_ARMOR]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]
	[SOLID_DENSITY:8250]
	[LIQUID_DENSITY:8020]
	[MOLAR_MASS:80000]
	[IMPACT_YIELD:602000]
	[IMPACT_FRACTURE:843500]
	[IMPACT_STRAIN_AT_YIELD:547]
	[COMPRESSIVE_YIELD:602000]
	[COMPRESSIVE_FRACTURE:843500]
	[COMPRESSIVE_STRAIN_AT_YIELD:547] no data, used 110
	[TENSILE_YIELD:172000]
	[TENSILE_FRACTURE:241000]
	[TENSILE_STRAIN_AT_YIELD:156] 110
	[TORSION_YIELD:172000]
	[TORSION_FRACTURE:241000]
	[TORSION_STRAIN_AT_YIELD:156]
	[SHEAR_YIELD:172000]
	[SHEAR_FRACTURE:241000]
	[SHEAR_STRAIN_AT_YIELD:156] no data, used 110
	[BENDING_YIELD:172000]
	[BENDING_FRACTURE:241000]
	[BENDING_STRAIN_AT_YIELD:156]
	[MAX_EDGE:10000]

[INORGANIC:BRASS]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:brass]
	[STATE_NAME_ADJ:LIQUID:molten brass]
	[STATE_NAME_ADJ:GAS:boiling brass]
	[DISPLAY_COLOR:6:6:1]
	[MATERIAL_VALUE:7]
	[SPEC_HEAT:377]
	[MELTING_POINT:11656]
	[BOILING_POINT:14068]
	[SOLID_DENSITY:8550]
	[LIQUID_DENSITY:8000]
	[MOLAR_MASS:64000]
	[IMPACT_YIELD:290500]
	[IMPACT_FRACTURE:1015000]
	[IMPACT_STRAIN_AT_YIELD:264]
	[COMPRESSIVE_YIELD:290500]
	[COMPRESSIVE_FRACTURE:1015000]
	[COMPRESSIVE_STRAIN_AT_YIELD:264] no data, used 110
	[TENSILE_YIELD:83000]
	[TENSILE_FRACTURE:290000]
	[TENSILE_STRAIN_AT_YIELD:75] 110
	[TORSION_YIELD:83000]
	[TORSION_FRACTURE:299000]
	[TORSION_STRAIN_AT_YIELD:75]
	[SHEAR_YIELD:83000]
	[SHEAR_FRACTURE:290000]
	[SHEAR_STRAIN_AT_YIELD:75] no data, used 110
	[BENDING_YIELD:83000]
	[BENDING_FRACTURE:290000]
	[BENDING_STRAIN_AT_YIELD:75]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:STEEL]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:steel]
	[STATE_NAME_ADJ:LIQUID:molten steel]
	[STATE_NAME_ADJ:GAS:boiling steel]
	[DISPLAY_COLOR:0:7:1]
	[MATERIAL_VALUE:30]
	[SPEC_HEAT:500]
	[MELTING_POINT:12718]
	[BOILING_POINT:14968]
	[ITEMS_WEAPON][ITEMS_WEAPON_RANGED][ITEMS_AMMO][ITEMS_DIGGER][ITEMS_ARMOR][ITEMS_ANVIL]
	[SOLID_DENSITY:7850]
	[LIQUID_DENSITY:6980]
	[MOLAR_MASS:55845]
	[IMPACT_YIELD:1505000]
	[IMPACT_FRACTURE:2520000]
	[IMPACT_STRAIN_AT_YIELD:940]
	[COMPRESSIVE_YIELD:1505000]
	[COMPRESSIVE_FRACTURE:2520000]
	[COMPRESSIVE_STRAIN_AT_YIELD:940] 160
	[TENSILE_YIELD:430000]
	[TENSILE_FRACTURE:720000]
	[TENSILE_STRAIN_AT_YIELD:225] 200
	[TORSION_YIELD:430000]
	[TORSION_FRACTURE:720000]
	[TORSION_STRAIN_AT_YIELD:215]
	[SHEAR_YIELD:430000]
	[SHEAR_FRACTURE:720000]
	[SHEAR_STRAIN_AT_YIELD:215] no data, used 200
	[BENDING_YIELD:430000]
	[BENDING_FRACTURE:720000]
	[BENDING_STRAIN_AT_YIELD:215]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:PIG_IRON]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:pig iron]
	[STATE_NAME_ADJ:LIQUID:molten pig iron]
	[STATE_NAME_ADJ:GAS:boiling pig iron]
	[DISPLAY_COLOR:0:7:1]
	[MATERIAL_VALUE:10]
	[SPEC_HEAT:500]
	[MELTING_POINT:12106]
	[BOILING_POINT:13968]
	[SOLID_DENSITY:7850]
	[LIQUID_DENSITY:6980]
	[MOLAR_MASS:55845]
	[IMPACT_YIELD:455000]
	[IMPACT_FRACTURE:700000]
	[IMPACT_STRAIN_AT_YIELD:268]
	[COMPRESSIVE_YIELD:455000]
	[COMPRESSIVE_FRACTURE:700000]
	[COMPRESSIVE_STRAIN_AT_YIELD:268]
	[TENSILE_YIELD:130000]
	[TENSILE_FRACTURE:200000]
	[TENSILE_STRAIN_AT_YIELD:62]
	[TORSION_YIELD:130000]
	[TORSION_FRACTURE:200000]
	[TORSION_STRAIN_AT_YIELD:159]
	[SHEAR_YIELD:130000]
	[SHEAR_FRACTURE:200000]
	[SHEAR_STRAIN_AT_YIELD:159]
	[BENDING_YIELD:130000]
	[BENDING_FRACTURE:200000]
	[BENDING_STRAIN_AT_YIELD:62]
	[MAX_EDGE:10000]

[INORGANIC:PLATINUM]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:platinum]
	[STATE_NAME_ADJ:LIQUID:molten platinum]
	[STATE_NAME_ADJ:GAS:boiling platinum]
	[DISPLAY_COLOR:7:7:1]
	[MATERIAL_VALUE:40]
	[SPEC_HEAT:130]
	[MELTING_POINT:13182]
	[BOILING_POINT:16885]
	[SOLID_DENSITY:21400]
	[LIQUID_DENSITY:19770]
	[MOLAR_MASS:195084]
	[IMPACT_YIELD:350000]
	[IMPACT_FRACTURE:700000]
	[IMPACT_STRAIN_AT_YIELD:152]
	[COMPRESSIVE_YIELD:350000]
	[COMPRESSIVE_FRACTURE:700000]
	[COMPRESSIVE_STRAIN_AT_YIELD:152] 230
	[TENSILE_YIELD:100000]
	[TENSILE_FRACTURE:200000]
	[TENSILE_STRAIN_AT_YIELD:60] 168
	[TORSION_YIELD:100000]
	[TORSION_FRACTURE:200000]
	[TORSION_STRAIN_AT_YIELD:164]
	[SHEAR_YIELD:100000]
	[SHEAR_FRACTURE:200000]
	[SHEAR_STRAIN_AT_YIELD:164] 61
	[BENDING_YIELD:100000]
	[BENDING_FRACTURE:200000]
	[BENDING_STRAIN_AT_YIELD:60]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:ELECTRUM]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:electrum]
	[STATE_NAME_ADJ:LIQUID:molten electrum]
	[STATE_NAME_ADJ:GAS:boiling electrum]
	[DISPLAY_COLOR:6:6:1]
	[MATERIAL_VALUE:20]
	[SPEC_HEAT:180]
	[MELTING_POINT:11828]
	[BOILING_POINT:14968]
	[SOLID_DENSITY:15000]
	[LIQUID_DENSITY:13000]
	[MOLAR_MASS:150000]
	Used gold.
	[IMPACT_YIELD:175000]
	[IMPACT_FRACTURE:350000]
	[IMPACT_STRAIN_AT_YIELD:97]
	[COMPRESSIVE_YIELD:175000]
	[COMPRESSIVE_FRACTURE:350000]
	[COMPRESSIVE_STRAIN_AT_YIELD:97] bulk modulus 180 GPa
	[TENSILE_YIELD:50000]
	[TENSILE_FRACTURE:100000]
	[TENSILE_STRAIN_AT_YIELD:64] young's modulus 78 GPa
	[TORSION_YIELD:50000]
	[TORSION_FRACTURE:100000]
	[TORSION_STRAIN_AT_YIELD:185]
	[SHEAR_YIELD:50000]
	[SHEAR_FRACTURE:100000]
	[SHEAR_STRAIN_AT_YIELD:185] shear modulus 27 GPa
	[BENDING_YIELD:50000]
	[BENDING_FRACTURE:100000]
	[BENDING_STRAIN_AT_YIELD:64]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:TIN]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:tin]
	[STATE_NAME_ADJ:LIQUID:molten tin]
	[STATE_NAME_ADJ:GAS:boiling tin]
	[DISPLAY_COLOR:7:3:0]
	[MATERIAL_VALUE:2]
	[SPEC_HEAT:210]
	[MELTING_POINT:10417]
	[BOILING_POINT:14684]
	[SOLID_DENSITY:7280]
	[LIQUID_DENSITY:6990]
	[MOLAR_MASS:118710]
	[IMPACT_YIELD:42000]
	[IMPACT_FRACTURE:350000]
	[IMPACT_STRAIN_AT_YIELD:724]
	[COMPRESSIVE_YIELD:42000]
	[COMPRESSIVE_FRACTURE:350000]
	[COMPRESSIVE_STRAIN_AT_YIELD:724] 58
	[TENSILE_YIELD:12000]
	[TENSILE_FRACTURE:100000]
	[TENSILE_STRAIN_AT_YIELD:24] 50
	[TORSION_YIELD:12000]
	[TORSION_FRACTURE:100000]
	[TORSION_STRAIN_AT_YIELD:66]
	[SHEAR_YIELD:12000]
	[SHEAR_FRACTURE:100000]
	[SHEAR_STRAIN_AT_YIELD:66] 18
	[BENDING_YIELD:12000]
	[BENDING_FRACTURE:100000]
	[BENDING_STRAIN_AT_YIELD:24]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:PEWTER_FINE]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:fine pewter]
	[STATE_NAME_ADJ:LIQUID:molten fine pewter]
	[STATE_NAME_ADJ:GAS:boiling fine pewter]
	[DISPLAY_COLOR:7:7:1]
	[MATERIAL_VALUE:5]
	[SPEC_HEAT:210]
	[MELTING_POINT:10417]
	[BOILING_POINT:14684]
	[SOLID_DENSITY:7280]
	[LIQUID_DENSITY:6990]
	[MOLAR_MASS:118710]
	[IMPACT_YIELD:42000]
	[IMPACT_FRACTURE:350000]
	[IMPACT_STRAIN_AT_YIELD:724]
	[COMPRESSIVE_YIELD:42000]
	[COMPRESSIVE_FRACTURE:350000]
	[COMPRESSIVE_STRAIN_AT_YIELD:724] 58
	[TENSILE_YIELD:12000]
	[TENSILE_FRACTURE:100000]
	[TENSILE_STRAIN_AT_YIELD:24] 50
	[TORSION_YIELD:12000]
	[TORSION_FRACTURE:100000]
	[TORSION_STRAIN_AT_YIELD:66]
	[SHEAR_YIELD:12000]
	[SHEAR_FRACTURE:100000]
	[SHEAR_STRAIN_AT_YIELD:66] 18
	[BENDING_YIELD:12000]
	[BENDING_FRACTURE:100000]
	[BENDING_STRAIN_AT_YIELD:24]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:PEWTER_TRIFLE]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:trifle pewter]
	[STATE_NAME_ADJ:LIQUID:molten trifle pewter]
	[STATE_NAME_ADJ:GAS:boiling trifle pewter]
	[DISPLAY_COLOR:7:3:0]
	[MATERIAL_VALUE:4]
	[SPEC_HEAT:210]
	[MELTING_POINT:10417]
	[BOILING_POINT:14684]
	[SOLID_DENSITY:7280]
	[LIQUID_DENSITY:6990]
	[MOLAR_MASS:118710]
	[IMPACT_YIELD:42000]
	[IMPACT_FRACTURE:350000]
	[IMPACT_STRAIN_AT_YIELD:724]
	[COMPRESSIVE_YIELD:42000]
	[COMPRESSIVE_FRACTURE:350000]
	[COMPRESSIVE_STRAIN_AT_YIELD:724] 58
	[TENSILE_YIELD:12000]
	[TENSILE_FRACTURE:100000]
	[TENSILE_STRAIN_AT_YIELD:24] 50
	[TORSION_YIELD:12000]
	[TORSION_FRACTURE:100000]
	[TORSION_STRAIN_AT_YIELD:66]
	[SHEAR_YIELD:12000]
	[SHEAR_FRACTURE:100000]
	[SHEAR_STRAIN_AT_YIELD:66] 18
	[BENDING_YIELD:12000]
	[BENDING_FRACTURE:100000]
	[BENDING_STRAIN_AT_YIELD:24]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:PEWTER_LAY]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:lay pewter]
	[STATE_NAME_ADJ:LIQUID:molten lay pewter]
	[STATE_NAME_ADJ:GAS:boiling lay pewter]
	[DISPLAY_COLOR:3:7:0]
	[MATERIAL_VALUE:3]
	[SPEC_HEAT:210]
	[MELTING_POINT:10417]
	[BOILING_POINT:14684]
	[SOLID_DENSITY:7280]
	[LIQUID_DENSITY:6990]
	[MOLAR_MASS:118710]
	[IMPACT_YIELD:42000]
	[IMPACT_FRACTURE:350000]
	[IMPACT_STRAIN_AT_YIELD:724]
	[COMPRESSIVE_YIELD:42000]
	[COMPRESSIVE_FRACTURE:350000]
	[COMPRESSIVE_STRAIN_AT_YIELD:724] 58
	[TENSILE_YIELD:12000]
	[TENSILE_FRACTURE:100000]
	[TENSILE_STRAIN_AT_YIELD:24] 50
	[TORSION_YIELD:12000]
	[TORSION_FRACTURE:100000]
	[TORSION_STRAIN_AT_YIELD:66]
	[SHEAR_YIELD:12000]
	[SHEAR_FRACTURE:100000]
	[SHEAR_STRAIN_AT_YIELD:66] 18
	[BENDING_YIELD:12000]
	[BENDING_FRACTURE:100000]
	[BENDING_STRAIN_AT_YIELD:24]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:LEAD]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:lead]
	[STATE_NAME_ADJ:LIQUID:molten lead]
	[STATE_NAME_ADJ:GAS:boiling lead]
	[DISPLAY_COLOR:0:7:1]
	[MATERIAL_VALUE:2]
	[SPEC_HEAT:130]
	[MELTING_POINT:10589]
	[BOILING_POINT:13148]
	[SOLID_DENSITY:11340]
	[LIQUID_DENSITY:10660]
	[MOLAR_MASS:207200]
	[IMPACT_YIELD:35000]
	[IMPACT_FRACTURE:42000]
	[IMPACT_STRAIN_AT_YIELD:760]
	[COMPRESSIVE_YIELD:35000]
	[COMPRESSIVE_FRACTURE:42000]
	[COMPRESSIVE_STRAIN_AT_YIELD:760] 46
	[TENSILE_YIELD:10000]
	[TENSILE_FRACTURE:12000]
	[TENSILE_STRAIN_AT_YIELD:63] 16
	[TORSION_YIELD:10000]
	[TORSION_FRACTURE:12000]
	[TORSION_STRAIN_AT_YIELD:179]
	[SHEAR_YIELD:10000]
	[SHEAR_FRACTURE:12000]
	[SHEAR_STRAIN_AT_YIELD:179] 5.6
	[BENDING_YIELD:10000]
	[BENDING_FRACTURE:12000]
	[BENDING_STRAIN_AT_YIELD:63]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:ALUMINUM]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:aluminum]
	[STATE_NAME_ADJ:LIQUID:molten aluminum]
	[STATE_NAME_ADJ:GAS:boiling aluminum]
	[DISPLAY_COLOR:7:7:1]
	[MATERIAL_VALUE:40]
	[SPEC_HEAT:900]
	[MELTING_POINT:11188]
	[BOILING_POINT:14534]
	[SOLID_DENSITY:2700]
	[LIQUID_DENSITY:2375]
	[MOLAR_MASS:26981]
	[IMPACT_YIELD:70000]
	[IMPACT_FRACTURE:175000]
	[IMPACT_STRAIN_AT_YIELD:921]
	[COMPRESSIVE_YIELD:70000]
	[COMPRESSIVE_FRACTURE:175000]
	[COMPRESSIVE_STRAIN_AT_YIELD:921] 76
	[TENSILE_YIELD:20000]
	[TENSILE_FRACTURE:50000]
	[TENSILE_STRAIN_AT_YIELD:29] 70
	[TORSION_YIELD:20000]
	[TORSION_FRACTURE:50000]
	[TORSION_STRAIN_AT_YIELD:77]
	[SHEAR_YIELD:20000]
	[SHEAR_FRACTURE:50000]
	[SHEAR_STRAIN_AT_YIELD:77] 26
	[BENDING_YIELD:20000]
	[BENDING_FRACTURE:50000]
	[BENDING_STRAIN_AT_YIELD:29]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

temperature values unknown, used nickel
[INORGANIC:NICKEL_SILVER]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:nickel silver]
	[STATE_NAME_ADJ:LIQUID:molten nickel silver]
	[STATE_NAME_ADJ:GAS:boiling nickel silver]
	[DISPLAY_COLOR:7:7:1]
	[MATERIAL_VALUE:3]
	[SPEC_HEAT:444]
	[MELTING_POINT:11620] german wiki
	[BOILING_POINT:15243]
	[SOLID_DENSITY:8650]
	[LIQUID_DENSITY:7810]
	[MOLAR_MASS:58693]
	[IMPACT_YIELD:70000]
	[IMPACT_FRACTURE:560000]
	[IMPACT_STRAIN_AT_YIELD:388]
	[COMPRESSIVE_YIELD:70000]
	[COMPRESSIVE_FRACTURE:560000]
	[COMPRESSIVE_STRAIN_AT_YIELD:388] 180
	[TENSILE_YIELD:20000]
	[TENSILE_FRACTURE:160000]
	[TENSILE_STRAIN_AT_YIELD:10] 200
	[TORSION_YIELD:20000]
	[TORSION_FRACTURE:160000]
	[TORSION_STRAIN_AT_YIELD:26]
	[SHEAR_YIELD:20000]
	[SHEAR_FRACTURE:160000]
	[SHEAR_STRAIN_AT_YIELD:26] 76
	[BENDING_YIELD:20000]
	[BENDING_FRACTURE:160000]
	[BENDING_STRAIN_AT_YIELD:10]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

temperature values unknown, used copper
[INORGANIC:BILLON]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:billon]
	[STATE_NAME_ADJ:LIQUID:molten billon]
	[STATE_NAME_ADJ:GAS:boiling billon]
	[DISPLAY_COLOR:7:3:0]
	[MATERIAL_VALUE:6]
	[SPEC_HEAT:385]
	[MELTING_POINT:11952]
	[BOILING_POINT:14611]
	[SOLID_DENSITY:8930] used copper
	[LIQUID_DENSITY:8020]
	[MOLAR_MASS:63546]
	[IMPACT_YIELD:245000]
	[IMPACT_FRACTURE:770000]
	[IMPACT_STRAIN_AT_YIELD:175]
	[COMPRESSIVE_YIELD:245000]
	[COMPRESSIVE_FRACTURE:770000]
	[COMPRESSIVE_STRAIN_AT_YIELD:175] 140
	[TENSILE_YIELD:70000]
	[TENSILE_FRACTURE:220000]
	[TENSILE_STRAIN_AT_YIELD:58] 120
	[TORSION_YIELD:70000]
	[TORSION_FRACTURE:220000]
	[TORSION_STRAIN_AT_YIELD:145]
	[SHEAR_YIELD:70000]
	[SHEAR_FRACTURE:220000]
	[SHEAR_STRAIN_AT_YIELD:145] 48
	[BENDING_YIELD:70000]
	[BENDING_FRACTURE:220000]
	[BENDING_STRAIN_AT_YIELD:58]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

temperature values unknown, used silver
value is weighted average of 3 silver and 1 copper
[INORGANIC:STERLING_SILVER]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:sterling silver]
	[STATE_NAME_ADJ:LIQUID:molten sterling silver]
	[STATE_NAME_ADJ:GAS:boiling sterling silver]
	[DISPLAY_COLOR:7:7:1]
	[MATERIAL_VALUE:8]
	[SPEC_HEAT:230]
	[MELTING_POINT:11602] unknown source
	[BOILING_POINT:13892]
	[SOLID_DENSITY:10490] used silver
	[LIQUID_DENSITY:9320]
	[MOLAR_MASS:107868]
	[IMPACT_YIELD:350000]
	[IMPACT_FRACTURE:595000]
	[IMPACT_STRAIN_AT_YIELD:350]
	[COMPRESSIVE_YIELD:350000]
	[COMPRESSIVE_FRACTURE:595000]
	[COMPRESSIVE_STRAIN_AT_YIELD:350] 100
	[TENSILE_YIELD:100000]
	[TENSILE_FRACTURE:170000]
	[TENSILE_STRAIN_AT_YIELD:120] 83
	[TORSION_YIELD:100000]
	[TORSION_FRACTURE:170000]
	[TORSION_STRAIN_AT_YIELD:333]
	[SHEAR_YIELD:100000]
	[SHEAR_FRACTURE:170000]
	[SHEAR_STRAIN_AT_YIELD:333] 30
	[BENDING_YIELD:100000]
	[BENDING_FRACTURE:170000]
	[BENDING_ELASTICITY:120]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

temperature values unknown, used copper
also called shakudo or hepatizon depending on the proportions (some have no silver)
	got the name from black corinthian bronze, though these proportions are more like regular corinthian bronze/brass
		I just wanted the liver-colored one, dropped "corinthian" because it sounds too location/culture specific
value of 11 is the weighted average value of 2copper/1silver/1gold components
[INORGANIC:BLACK_BRONZE]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:black bronze]
	[STATE_NAME_ADJ:LIQUID:molten black bronze]
	[STATE_NAME_ADJ:GAS:boiling black bronze]
	[DISPLAY_COLOR:5:6:0]
	[MATERIAL_VALUE:11]
	[SPEC_HEAT:385]
	[MELTING_POINT:11952]
	[BOILING_POINT:14611]
	[SOLID_DENSITY:8930]
	[LIQUID_DENSITY:8020]
	[MOLAR_MASS:63546]
	[IMPACT_YIELD:245000]
	[IMPACT_FRACTURE:770000]
	[IMPACT_STRAIN_AT_YIELD:175]
	[COMPRESSIVE_YIELD:245000]
	[COMPRESSIVE_FRACTURE:770000]
	[COMPRESSIVE_STRAIN_AT_YIELD:175] 140
	[TENSILE_YIELD:70000]
	[TENSILE_FRACTURE:220000]
	[TENSILE_STRAIN_AT_YIELD:58] 120
	[TORSION_YIELD:70000]
	[TORSION_FRACTURE:220000]
	[TORSION_STRAIN_AT_YIELD:145]
	[SHEAR_YIELD:70000]
	[SHEAR_FRACTURE:220000]
	[SHEAR_STRAIN_AT_YIELD:145] 48
	[BENDING_YIELD:70000]
	[BENDING_FRACTURE:220000]
	[BENDING_STRAIN_AT_YIELD:58]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

temperature values unknown, used gold
value is weighted average of 3 gold and 1 copper
[INORGANIC:ROSE_GOLD]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:rose gold]
	[STATE_NAME_ADJ:LIQUID:molten rose gold]
	[STATE_NAME_ADJ:GAS:boiling rose gold]
	[DISPLAY_COLOR:5:5:1]
	[MATERIAL_VALUE:23]
	[SPEC_HEAT:129]
	[MELTING_POINT:11915]
	[BOILING_POINT:15141]
	[SOLID_DENSITY:19320] used gold
	[LIQUID_DENSITY:17310]
	[MOLAR_MASS:196967]
	[IMPACT_YIELD:175000]
	[IMPACT_FRACTURE:350000]
	[IMPACT_STRAIN_AT_YIELD:97]
	[COMPRESSIVE_YIELD:175000]
	[COMPRESSIVE_FRACTURE:350000]
	[COMPRESSIVE_STRAIN_AT_YIELD:97] bulk modulus 180 GPa
	[TENSILE_YIELD:50000]
	[TENSILE_FRACTURE:100000]
	[TENSILE_STRAIN_AT_YIELD:64] young's modulus 78 GPa
	[TORSION_YIELD:50000]
	[TORSION_FRACTURE:100000]
	[TORSION_STRAIN_AT_YIELD:185]
	[SHEAR_YIELD:50000]
	[SHEAR_FRACTURE:100000]
	[SHEAR_STRAIN_AT_YIELD:185] shear modulus 27 GPa
	[BENDING_YIELD:50000]
	[BENDING_FRACTURE:100000]
	[BENDING_STRAIN_AT_YIELD:64]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

bismuth itself is brittle, but you can alloy it with tin/copper to make a light-colored bronze
[INORGANIC:BISMUTH]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:bismuth]
	[STATE_NAME_ADJ:LIQUID:molten bismuth]
	[STATE_NAME_ADJ:GAS:boiling bismuth]
	[DISPLAY_COLOR:5:5:1]
	[MATERIAL_VALUE:2]
	[SPEC_HEAT:123]
	[MELTING_POINT:10488]
	[BOILING_POINT:12815]
	[SOLID_DENSITY:9780]
	[LIQUID_DENSITY:10050]
	[MOLAR_MASS:208980]
	[IMPACT_YIELD:105000]
	[IMPACT_FRACTURE:175000]
	[IMPACT_STRAIN_AT_YIELD:3387]
	[COMPRESSIVE_YIELD:105000]
	[COMPRESSIVE_FRACTURE:175000]
	[COMPRESSIVE_STRAIN_AT_YIELD:3387] 31
	[TENSILE_YIELD:30000]
	[TENSILE_FRACTURE:50000]
	[TENSILE_STRAIN_AT_YIELD:94] 32
	[TORSION_YIELD:30000]
	[TORSION_FRACTURE:50000]
	[TORSION_STRAIN_AT_YIELD:250]
	[SHEAR_YIELD:30000]
	[SHEAR_FRACTURE:50000]
	[SHEAR_STRAIN_AT_YIELD:250] 12
	[BENDING_YIELD:30000]
	[BENDING_FRACTURE:50000]
	[BENDING_STRAIN_AT_YIELD:94]
	[MAX_EDGE:10000]

you can make a lighter colored bronze by adding bismuth, used temp values from bronze, used by incas, at least according to one source ha ha
[INORGANIC:BISMUTH_BRONZE]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:bismuth bronze]
	[STATE_NAME_ADJ:LIQUID:molten bismuth bronze]
	[STATE_NAME_ADJ:GAS:boiling bismuth bronze]
	[DISPLAY_COLOR:6:6:1]
	[MATERIAL_VALUE:6]
	[SPEC_HEAT:435]
	[MELTING_POINT:11868]
	[BOILING_POINT:14140]
	[ITEMS_WEAPON][ITEMS_WEAPON_RANGED][ITEMS_AMMO][ITEMS_DIGGER][ITEMS_ARMOR]
	[SOLID_DENSITY:8250] used bronze
	[LIQUID_DENSITY:8020]
	[MOLAR_MASS:80000]
	[IMPACT_YIELD:602000]
	[IMPACT_FRACTURE:843500]
	[IMPACT_STRAIN_AT_YIELD:547]
	[COMPRESSIVE_YIELD:602000]
	[COMPRESSIVE_FRACTURE:843500]
	[COMPRESSIVE_STRAIN_AT_YIELD:547] no data, used 110
	[TENSILE_YIELD:172000]
	[TENSILE_FRACTURE:241000]
	[TENSILE_STRAIN_AT_YIELD:156] 110
	[TORSION_YIELD:172000]
	[TORSION_FRACTURE:241000]
	[TORSION_STRAIN_AT_YIELD:156]
	[SHEAR_YIELD:172000]
	[SHEAR_FRACTURE:241000]
	[SHEAR_STRAIN_AT_YIELD:156] no data, used 110
	[BENDING_YIELD:172000]
	[BENDING_FRACTURE:241000]
	[BENDING_STRAIN_AT_YIELD:156]
	[MAX_EDGE:10000]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]

[INORGANIC:ADAMANTINE]
	[USE_MATERIAL_TEMPLATE:METAL_TEMPLATE]
	[STATE_NAME_ADJ:ALL_SOLID:adamantine]
	[STATE_NAME_ADJ:LIQUID:molten adamantine]
	[STATE_NAME_ADJ:GAS:boiling adamantine]
	[DISPLAY_COLOR:3:3:1]
	[MATERIAL_VALUE:300]
	[SPEC_HEAT:7500]
	[MELTING_POINT:25000]
	[BOILING_POINT:50000]
	[ITEMS_WEAPON][ITEMS_WEAPON_RANGED][ITEMS_AMMO][ITEMS_DIGGER][ITEMS_ARMOR][ITEMS_ANVIL]
	[ITEMS_HARD]
	[ITEMS_METAL]
	[ITEMS_BARRED]
	[ITEMS_SCALED]
	[ITEMS_SOFT]
	[WAFERS]
	[SOLID_DENSITY:200]
	[LIQUID_DENSITY:2600]
	[MOLAR_MASS:55845]
	[IMPACT_YIELD:5000000]
	[IMPACT_FRACTURE:5000000]
	[IMPACT_STRAIN_AT_YIELD:0]
	[COMPRESSIVE_YIELD:5000000]
	[COMPRESSIVE_FRACTURE:5000000]
	[COMPRESSIVE_STRAIN_AT_YIELD:0]
	[TENSILE_YIELD:5000000]
	[TENSILE_FRACTURE:5000000]
	[TENSILE_STRAIN_AT_YIELD:0]
	[TORSION_YIELD:5000000]
	[TORSION_FRACTURE:5000000]
	[TORSION_STRAIN_AT_YIELD:0]
	[SHEAR_YIELD:5000000]
	[SHEAR_FRACTURE:5000000]
	[SHEAR_STRAIN_AT_YIELD:0]
	[BENDING_YIELD:5000000]
	[BENDING_FRACTURE:5000000]
	[BENDING_STRAIN_AT_YIELD:0]
	[MAX_EDGE:100000]
	[DEEP_SPECIAL]
	[STOCKPILE_THREAD_METAL]